Updating the firmware on Dreamoc POP and Scandinavia 180/360 players

1. Copy the firmware image file onto the SD card. You do not have to erase other files on the card.
2. Insert the SD card properly in the player.
3. Turn on power.
4. Once a movie starts playing push the stop button to access the menu (If there is no movie on the card the menu will appear once the unit is ready).
5. Use the left arrow button and highlight the explorer icon (far left icon).
6. Push the enter button.
7. Choose the SD card module and push enter again.
8. Confirm the SD card in the slot by pushing enter a third time.
9. Now locate the firmware file using the up and down arrows and activate it with the enter button.
10. Confirm that you wish to update the firmware by pushing enter a last time.
11. DO NOT TURN OF THE PLAYER WHILE IT IS UPDATING!
12. Wait while the firmware is being updated. The player will automatically restart during this process, and it will take around 20 seconds before it turns on again.
13. When the player starts again the process is complete and the firmware is updated.